**,**

**Helmer TC 31 Anti Bark Collar User s Manual**

Introduction:

The Anti-Bark Collar stops barking with progressively increasing sound and shock which is controlled by a microprocessor distinguishing your dog's bark from other

Principles of operation:

At the first bark, TC 31 Anti-bark Collar applies a short warning tone. If a second bark occurs within thirty seconds, a more intense tone is sounded. From the third bark, a more intense tone

This pattern is repeated through 7 correction levels. The first two levels are only with progressively warning tone. If your dog continues to bark through the rest five levels, the more intense sound and shock are applies after each bark until your pet stops for thirty seconds, and then Anti-Bark Collar will automatically resets to the first "tone only" level of correction. To protect the dog, if the

The use of the warning tone followed by increasingly intense tones and shocks sets up a pattern that your dog will quickly learn is caused by its own barking. It takes time to break bad

When your dog forgets and barks again, the warning tone reminds your pet without immediately applying painful stimulus. At each step, your dog gets to choose whether it's worth the increasing pain to bark again. We have found this technique of progressively increasing sound and shock is not only more humane, it is more EFFECTIVE in breaking the barking habit

TC 31 can be adjusted to control the sensitivity of the voice, according to the size of dogs barking.

Operating Instructions:

Our TC 31 is almost completely automatic. Just install a 6 volt alkaline battery, adjust the strap to the size of your dog's neck and the TC 31 automatically begins doing its job.

There are two BUTTONS used to adjust the sensitivity to the bark, and every time there will be "B" out of tone, sensitivity will gradually be enhanced or weakened. The more sensitive, the easier to trigger the collar.

Installing/Replacing the Battery:

Take off the battery cover and make sure you install the battery correctly.

Install the new battery between the "clip" and "spring" contacts. Note that "spring" contact is for

the negative end and "clip" contact is for the positive end shown below.

Putting Anti-bark Collar on Your Dog.

Place the unit around your dog's neck and adjust the collar length using the slide buckle

arrangement provides with the strap. The unit should fit snugly underneath your dog's neck.

Battery Cover

Slide Open

Make sure that the electrodes are in the direct contact with your dog's skin. Hair between the

electrodes and skin will severely diminish the shock effect, If necessary, it is advisable to clip or

shave your don's fur under the neck to insure direct contact.

Caution Notes:

. Do not allow your dog to chew this collar. You should also attempt to minimize scratching or

1

clawing at the casing.

2

. This device is made up of plastic and electronic components that are not digestible. Consult

your local vet if your dog swallows any part of this product.

3

. The collar is not intended for use as a restraining collar. If you are using a leash, use it with a

separate restraining type of collar.

4

. Although the Anti-bark Collar's microprocessor is designed to differentiate your dog's

individual bark from stray environmental noises, the unit may occasionally be activated by

other vibrations or sounds.

This is normal but, it should not happen so often as to be confusing to your pet. If the unit is falsely

triggered by excessive scratching, shaking of the head or rolling on the ground, your pet may be

suffering from fleas or ear mites. If these activities are evident, have you pet checked by a

veterinarian for parasites.

Shock Electrodes

Sensitivity Level Dial

High

Low

Indication Light